**Article ID:** 1048

**Article Name:** Washing Machine door gasket is twisted and leaking

**Topic Location:** Laundry / Washer dryer / Door

**Meta-data:** door, leaking, seal, twisted, gasket

**Related Articles:**

**Related Questions:**

PNC

DIY

Safety

Link

Email

Book Engineer

Multimedia

Brand

**Article Content:**

Damaged door seal is normally caused by overloading or when clothes have been between seal and door glass in the beginning of a wash programme. A twisted, damaged, deformed or leaking seal has to be fixed or replaced by an authorized technician/engineer.

Please book an engineer and don’t use the appliances until the problem is fixed.

To book a certified/authorized Electrolux technician/engineer please

* use our online-booking: tbd.
* or call us: tbd.
* or use our contact-webform: tbd.
* or send us an E-mail to: tbd.