|  |  |
| --- | --- |
| **Article ID:** | 2058 |
| **Article Name:** | [2058]My oven is not holding the required temperature |
| **Topic Location:** | Cooking/Oven/Usage/Performance |
| **Meta-data:** | Temperature, wrong, not holding |
| **Related Articles:** |  |
| **Related Questions:** |  |

PNC

DIY

Safety

Link

Email

Book Engineer

Multimedia

Brand

**Article Content:**

Normally, when you select a temperature in your oven, it will start heating up until it reaches the selected temperature. Once this has been reached the heating elements will be disconnected and reconnected again when the temperature goes below the selected one. This graph shows you the behaviour of the heating elements during the cooking process.



[http://www.ezone-teams.electrolux.com/knowledgeteamcustcareemea/Authoring/Multimedia%20Files/Images/Pictures/Cooking/[2058]%20Temperature%20graph.jpg](http://www.ezone-teams.electrolux.com/knowledgeteamcustcareemea/Authoring/Multimedia%20Files/Images/Pictures/Cooking/%5b2058%5d%20Temperature%20graph.jpg)

If you are using the turbo function, also check that the inner fan on the back panel is running, if not this could cause the temperature not to be distributed throughout the cavity. Also check that the oveb door is closed correctly.

If neither of the previous points refers to your case, and the temperature of your oven is always lower than the selected one, it could well be a problem related to technical failure. In this case you should contact our service force for support, by clicking the link below:

[book\_engineer\_link]